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Project details
PROJECT
	Building
	Lindenhof apartments · Example

	Address
	Musterstraße 12, 12345 Musterstadt

	Example
	Fictional project · 18 October 2026


PARTICIPANTS
	Site manager
	Lena Weber · Lindenbau · Beispiel
lena.weber@lindenbau.example · +49 000 10001

	Planner
	Mara König · Planwerk · Beispiel
mara.koenig@planwerk.example · +49 000 10002

	Contractor
	Jonas Berger · Fassadenwerk · Beispiel
jonas.berger@fassadenwerk.example · +49 000 10003


Documentation details
INSPECTION
	Date
	18 Oct 2026

	Documentation number
	LH-2026-001

	Purpose
	Record visible building-envelope defects and define further investigation and follow-up.

	Property
	Lindenhof apartments - Musterstraße 12, 12345 Musterstadt

	Inspection time
	09:15-11:15

	Inspection method
	External visual inspection from accessible ground-level areas

	Prepared by
	Mara König - building surveyor

	Follow-up reviewed
	19 October 2026


INSPECTION PARTICIPANTS
	Planner
	Mara König · Planwerk · Beispiel
mara.koenig@planwerk.example · +49 000 10002

	Site manager
	Lena Weber · Lindenbau · Beispiel
lena.weber@lindenbau.example · +49 000 10001


[bookmark: qr_317288588daa2fea4798680e]Task overview
	Task
	Location
	Responsible
	Status
	Deadline
	Page

	Task 1 · Arrange assessment of the damaged balcony edge
	Pin 1.1.1 · Defect
	Lena Weber · Lindenbau · Beispiel
	In progress
	23 Oct 2026
	

	Task 2 · Measure moisture and inspect the downpipe connection
	Moisture
	Mara König · Planwerk · Beispiel
	Open · Overdue
	18 Oct 2026
	



[bookmark: qr_81a86f4e087d128cb1f3e5ab]Pin 1
[image: ]
[bookmark: qr_43d65331c1e50fad5e338d8a]Figure 1    ● Concrete damage
[bookmark: qr_fbe7ca8da63f2e2a30e00538]Pin 1.1
[image: ]
[bookmark: qr_2c82825506a259e8d0271daa]Figure 2
[bookmark: qr_eb87f69a837ec1e2d6330513]Pin 1.1.1 · Defect
	Component
	Concrete spalling · Balcony underside
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[bookmark: qr_1cefd9c6c3bfaca69e58f1ca]Figure 3 · Concrete spalling · Balcony underside
	Assessment and investigation - exposed reinforcement
The visible condition is consistent with deterioration of the concrete cover associated with reinforcement corrosion. The initiating cause and the extent of corrosion cannot be established by visual inspection. Further loose or detached concrete may be present beyond the visible opening.

A competent concrete specialist should inspect the underside and adjacent slab edges at close range, establish the extent of unsound concrete and assess cover and reinforcement condition. The slab top, waterproofing, edge details and drainage should also be checked for possible moisture entry. The specialist should determine any further testing and whether structural assessment is required.

Maintain the precautionary restriction below the affected area until it has been assessed. Define repair measures from the investigation findings; this visual record does not establish that the balcony is safe for unrestricted use.



TASKS AND MEASURES
[bookmark: qr_ca2ca41ef4989097f2acaa1a]Task 1 · Arrange assessment of the damaged balcony edge
	Responsible
	Lena Weber · Lindenbau · Beispiel

	Status
	In progress

	Deadline
	23 Oct 2026 (Europe/Berlin)

	Comments
	Access is secured. Coordinate the inspection with the specialist before defining the repair.

	Evidence
	Figure 3


[bookmark: qr_e1c04edd9e7ae759cc3dd206]Moisture
	Component
	Moisture at the plinth
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[bookmark: qr_ce09072234fdf664807dff55]Figure 4 · West elevation - downpipe and plinth
● Moisture-related findings
	Location and context - west plinth
The marked area is at the foot of the rainwater downpipe on the west elevation, close to the north-west corner. The overview records the relationship between the staining, downpipe, gravel strip and adjacent ground. The linked detail photograph records the surface condition.
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[bookmark: qr_ac4e3dedcd155e0a2cbd7864]Figure 5 · Moisture at the plinth
	Finding - staining and deposits at the plinth
At the west elevation, beside the rainwater downpipe near the north-west corner, irregular dark staining is visible in the rendered plinth. The affected area is approximately 0.60 m wide and extends to about 0.45 m above the adjoining ground level, estimated visually.

Patchy whitish deposits and local changes to the surface coating are visible. The boundary with the less affected render above is irregular. These features are compatible with repeated wetting and drying, but the deposits have not been identified by testing.

No material moisture measurements or inspection of the concealed wall layers was undertaken. Inspect the downpipe joints and drainage connection, adjacent ground levels and plinth detailing, then record comparative moisture readings before deciding on remedial work.



TASKS AND MEASURES
[bookmark: qr_b4103fcbea8c4c0ad05cf53d]Task 2 · Measure moisture and inspect the downpipe connection
	Responsible
	Mara König · Planwerk · Beispiel

	Status
	Open · Overdue

	Deadline
	18 Oct 2026 (Europe/Berlin)

	Comments
	Please add readings and a photo of the connection to this finding.

	Evidence
	Figure 5
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